; Localized	07/31/2002 10:00 AM (GMT+08:00)	2.0.0.0  ca536a.inf
; Composite Driver Information
; Copyright (c) 2002 Sunplus Tech
; Manufacturer: Sunplus Tech

[Version]
signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
Provider=%USBCamera%
LayoutFile=LAYOUT.INF
DriverVer=07/31/2002,2.0.0.0
;CatalogFile=CA536A.cat

[DestinationDirs]
DefaultDestDir=11               ; LDID_SYS

; =================== Class Sections ===========================

[ClassInstall]
Addreg=USBClassReg

[USBClassReg]
HKR,,,,%USBClassName%
HKR,,Icon,,-20


; =================== Table of content =========================

[Manufacturer]
%Sunplus.MfgName%=Sunplus.Section

[SourceDisksNames]
1="USB Camera Disk",USBCameraVideo,,

[SourceDisksFiles]
;CA5xxA.cat=1

; =================== Sunplus ==================================

[Sunplus.Section]
%CAMERA.DeviceDesc%=StandardHub.Dev,USB\VID_04FC&PID_5360


; =================== Global ==================================

[StandardHub.Dev]
AddReg=Hub.AddReg
CopyFiles=Hub.CopyFiles

[StandardHub.Dev.NT]
CopyFiles=Hub.CopyFiles.NT

[StandardHub.Dev.NT.Services]
AddService = usbhub, 0x00000002, StandardHub.AddService

[StandardHub.AddService]
DisplayName    = %StandardHub.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 2                  ; SERVICE_AUTO_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\usbhub.sys
LoadOrderGroup = Base

[HUB.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,usbhub.sys

[HUB.CopyFiles]

[USB.CopyFiles.NT]

[ControlFlags]

[DestinationDirs]
DefaultDestDir = 11             ; System directory

[Strings]
USBClassName= "Universal serial bus controller"
StandardHub.SvcDesc= "DSC Composite USB Device"

USBCamera=         "Sunplus"
Sunplus.MfgName=   "Sunplus"

CAMERA.DeviceDesc= "Icatch(VII) Composite USB Device"
