[Version]
Signature="$CHICAGO$"
Class=HDC
provider=%MSFT%

[Manufacturer]
%MfgName%=Microsoft

[Microsoft]
%USB\VID_054C&PID_0023.DeviceDesc%=SonyCDRW.install,USB\VID_55AA&PID_1234
%USB\VID_054C&PID_0023.DeviceDesc%=SonyCDRW.install,USB\VID_04CE&PID_0002
%USB\VID_04E6&PID_0001.DeviceDesc%=ImationLS120.install,USB\VID_04E6&PID_0001
%USB\VID_04fc&PID_1533.DeviceDesc%=SunplusIcatch.install,USB\VID_04fc&PID_1533
%USB\VID_04fc&PID_5361.DeviceDesc%=SunplusIcatch.install,USB\VID_04fc&PID_5361
%UMSS\DISK.DeviceDesc%=umsspdr.install,UMSS\DISK

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
; \<WINDIR>\SYSTEM32\DRIVERS
umss.files = 10,System32\Drivers

; \<WINDIR>\SYSTEM\IOSUBSYS
umsspdr.files = 12

[SonyCDRW.install]
CopyFiles=umss.files, umsspdr.files
AddReg=umss.addreg

[ImationLS120.install]
CopyFiles=umss.files, umsspdr.files
AddReg=umss.addreg

[ImationLS120.install.HW]
AddReg=cb.addreg.HW

[SunplusIcatch.install]
CopyFiles=umss.files, umsspdr.files
AddReg=umss.addreg

[SunplusIcatch.install.HW]
AddReg=bulkonly.addreg.HW

[umss.addreg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,UMSS.SYS


; Indicate that the device uses the C/B/I protocol
[cbi.addreg.HW]
HKR,,DeviceProtocol,0x10001,00

; Indicate that the device uses the C/B protocol
[cb.addreg.HW]
HKR,,DeviceProtocol,0x10001,01

; Indicate that the device uses the BULK ONLY protocol
[bulkonly.addreg.HW]
HKR,,DeviceProtocol,0x10001,50

; Install the port driver
[umsspdr.install]
AddReg=umsspdr.addreg

[umsspdr.addreg]
HKR,,DevLoader,,*ios
HKR,,PortDriver,,umsspdr.pdr



[umss.files]
umss.sys

[umsspdr.files]
umsspdr.pdr

[SourceDisksNames]
1000 = "USB Mass Storage Sample Driver Disk","",,

[SourceDisksFiles]
UMSS.SYS = 1000
UMSSPDR.PDR = 1000

;---------------------------------------------------------------;

[Strings]
MSFT="Microsoft"
MfgName="Microsoft"
USB\VID_054C&PID_0023.DeviceDesc="Sony USB CD-R/W Drive"
USB\VID_04E6&PID_0001.DeviceDesc="Imation USB LS-120 Drive"
USB\VID_04fc&PID_1533.DeviceDesc="Sunplus Icatch"
USB\VID_04fc&PID_5361.DeviceDesc="Sunplus Icatch"
UMSS\DISK.DeviceDesc="USB Mass Storage Device"
